(module Wafer_Vertical20x5.8x7RM2.5-7 (layer F.Cu) (tedit 556C2ABA)
  (descr "Gold-Tek vertical wafer connector with 2.5mm pitch")
  (tags "wafer connector vertical")
  (fp_text reference REF** (at 7.493 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Wafer_Vertical20x5.8x7RM2.5-7 (at 7.493 5.08) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.75 -2.75) (end 17.75 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.75 -2.75) (end 17.75 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.75 3.8) (end -2.75 3.8) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.75 3.8) (end -2.75 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.54 -2.413) (end -2.54 3.429) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 3.429) (end 17.526 3.429) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.526 3.429) (end 17.526 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.526 -2.413) (end -2.54 -2.413) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.493 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 4.993 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 7.493 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 9.993 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 12.493 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at 14.993 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model Connect.3dshapes/Wafer_Vertical20x5.8x7RM2.5-7.wrl
    (at (xyz 0 0 0))
    (scale (xyz 4 4 4))
    (rotate (xyz 0 0 0))
  )
)
