(module Wafer_Horizontal22.5x5.8x7RM2.5-8 (layer F.Cu) (tedit 556C2A63)
  (descr "Gold-Tek horizontal wafer connector with 2.5mm pitch")
  (tags "wafer connector horizontal")
  (fp_text reference REF** (at 8.89 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Wafer_Horizontal22.5x5.8x7RM2.5-8 (at 8.89 10.414) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.75 -2.75) (end 20.3 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 20.3 -2.75) (end 20.3 9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 20.3 9.65) (end -2.75 9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.75 9.65) (end -2.75 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 17.526 2.286) (end 17.526 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 20.066 -2.413) (end 18.796 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 18.796 -2.413) (end 18.796 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 -2.413) (end -1.27 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.27 -2.413) (end -1.27 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 2.286) (end 20.066 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 9.271) (end 20.066 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 9.271) (end -2.54 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.54 2.286) (end -2.54 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 20.066 2.286) (end 20.066 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 20.066 9.271) (end 20.066 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.891 9.271) (end 16.891 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.891 5.715) (end 18.161 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 18.161 5.715) (end 18.161 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 9.271) (end -0.508 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 5.715) (end 0.635 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.635 5.715) (end 0.635 9.144) (layer F.SilkS) (width 0.15))
  (fp_line (start 14.986 2.286) (end 14.986 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.573 2.286) (end 12.573 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.906 2.286) (end 9.906 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.493 2.286) (end 7.493 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.953 2.286) (end 4.953 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.54 2.286) (end 2.54 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 2.286) (end 0 1.397) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.513 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 5.013 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 7.513 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 10.013 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 12.513 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at 15.013 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 8 thru_hole circle (at 17.513 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model Connect.3dshapes/Wafer_Horizontal22.5x5.8x7RM2.5-8.wrl
    (at (xyz 0 0 0))
    (scale (xyz 4 4 4))
    (rotate (xyz 0 0 0))
  )
)
