(module SMB_Straight (layer F.Cu) (tedit 5541ED7C)
  (descr "SMB pcb mounting jack")
  (tags "SMB Jack  Striaght")
  (fp_text reference REF** (at -2 -5) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value SMB_Straight (at 0.25 0) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -4.25 -4.25) (end 4.25 -4.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start 4.25 -4.25) (end 4.25 4.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start 4.25 4.25) (end -4.25 4.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start -4.25 4.25) (end -4.25 -4.25) (layer B.CrtYd) (width 0.05))
  (fp_line (start 4.25 4.25) (end -4.25 4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 4.25) (end -4.25 -4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start 4.25 -4.25) (end 4.25 4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -4.25 -4.25) (end 4.25 -4.25) (layer F.CrtYd) (width 0.05))
  (fp_line (start -1 -3.5052) (end 1 -3.5052) (layer F.SilkS) (width 0.15))
  (fp_line (start 3.5052 -1) (end 3.5052 1) (layer F.SilkS) (width 0.15))
  (fp_line (start 1 3.5052) (end -1 3.5052) (layer F.SilkS) (width 0.15))
  (fp_line (start -3.5052 1) (end -3.5052 -1) (layer F.SilkS) (width 0.15))
  (pad 2 thru_hole circle (at -2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.54 2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at -2.54 -2.54) (size 2.74 2.74) (drill 1.7) (layers *.Cu *.Mask F.SilkS))
  (pad 1 thru_hole circle (at 0 0) (size 2.24 2.24) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model Connect.3dshapes/SMB_Straight.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
