(module Wafer_Horizontal20x5.8x7RM2.5-7 (layer F.Cu) (tedit 556C2A51)
  (descr "Gold-Tek horizontal wafer connector with 2.5mm pitch")
  (tags "wafer connector horizontal")
  (fp_text reference REF** (at 7.62 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Wafer_Horizontal20x5.8x7RM2.5-7 (at 7.62 10.414) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.5 -2.75) (end 18 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 18 -2.75) (end 18 9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 18 9.65) (end -2.5 9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.5 9.65) (end -2.5 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 14.351 9.271) (end 14.351 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 14.351 5.715) (end 15.621 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 15.621 5.715) (end 15.621 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 9.271) (end -0.508 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.508 5.715) (end 0.635 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.635 5.715) (end 0.635 9.144) (layer F.SilkS) (width 0.15))
  (fp_line (start 14.986 2.286) (end 14.986 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.573 2.286) (end 12.573 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.906 2.286) (end 9.906 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.493 2.286) (end 7.493 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.953 2.286) (end 4.953 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.54 2.286) (end 2.54 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 0 2.286) (end 0 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.653 2.413) (end 17.653 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.653 -2.413) (end 16.383 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 16.383 -2.413) (end 16.383 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 2.286) (end -2.286 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 -2.413) (end -1.397 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.397 -2.413) (end -1.397 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 2.286) (end 17.653 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.653 2.286) (end 17.653 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start 17.653 9.271) (end -2.286 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.286 9.271) (end -2.286 2.286) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.493 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 4.993 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 7.493 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 9.993 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 6 thru_hole circle (at 12.493 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 7 thru_hole circle (at 14.993 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model Connect.3dshapes/Wafer_Horizontal20x5.8x7RM2.5-7.wrl
    (at (xyz 0 0 0))
    (scale (xyz 4 4 4))
    (rotate (xyz 0 0 0))
  )
)
