(module USB_A_Vertical (layer F.Cu) (tedit 554409CC)
  (descr "USB A vertical female connector, right angle")
  (tags "USB_A_Vertical female connector angled 73725-0110BLF")
  (fp_text reference REF** (at 0 8.95) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value USB_A_Vertical (at -0.05 -5.8) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start 3.9 -12.75) (end 3.9 7.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3.9 7.55) (end -3.9 7.55) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.9 7.55) (end -3.9 -12.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start -3.9 -12.75) (end 3.9 -12.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 3 -1.82) (end 3 -12.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -1.82) (end -3 -12.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 -12.5) (end 3 -12.5) (layer F.SilkS) (width 0.15))
  (fp_line (start -3 0.36) (end -3 5.18) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.2 7.2735) (end -2.2 7.2735) (layer F.SilkS) (width 0.15))
  (fp_line (start 3 0.36) (end 3 5.18) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole circle (at 0 0) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask))
  (pad 2 thru_hole circle (at 0 2) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask))
  (pad 3 thru_hole circle (at 0 4) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 2.72 -0.73) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 0 6) (size 1.62 1.62) (drill 0.92) (layers *.Cu *.Mask))
  (pad 5 thru_hole circle (at 2.72 6.27) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -2.72 -0.73) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at -2.72 6.27) (size 1.85 1.85) (drill 1.35) (layers *.Cu *.Mask F.SilkS))
  (model Connect.3dshapes/USB_A_Vertical.wrl
    (at (xyz 0.015 -0.02 0.05))
    (scale (xyz 0.412 0.412 0.412))
    (rotate (xyz 0 -90 180))
  )
)
