(module Wafer_Horizontal15x5.8x7RM2.5-5 (layer F.Cu) (tedit 556C2A29)
  (descr "Gold-Tek horizontal wafer connector with 2.5mm pitch")
  (tags "wafer connector horizontal")
  (fp_text reference REF** (at 5.0165 -3.81) (layer F.SilkS)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_text value Wafer_Horizontal15x5.8x7RM2.5-5 (at 5.08 10.414) (layer F.Fab)
    (effects (font (size 1 1) (thickness 0.15)))
  )
  (fp_line (start -2.75 -2.75) (end 12.95 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.95 -2.75) (end 12.95 9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start 12.95 9.65) (end -2.75 9.65) (layer F.CrtYd) (width 0.05))
  (fp_line (start -2.75 9.65) (end -2.75 -2.75) (layer F.CrtYd) (width 0.05))
  (fp_line (start 10.0584 2.286) (end 10.0584 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 7.5184 2.159) (end 7.5184 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 4.9784 2.286) (end 4.9784 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 2.5654 1.397) (end 2.5654 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.0254 2.286) (end 0.0254 1.397) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.4234 9.271) (end 9.4234 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 9.4234 5.715) (end 10.6934 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 10.6934 5.715) (end 10.6934 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.6096 9.271) (end -0.6096 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start -0.6096 5.715) (end 0.6604 5.715) (layer F.SilkS) (width 0.15))
  (fp_line (start 0.6604 5.715) (end 0.6604 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.5984 2.286) (end 12.5984 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.5984 -2.413) (end 11.4554 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start 11.4554 -2.413) (end 11.4554 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5146 -2.413) (end -1.3716 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start -1.3716 -2.413) (end -1.3716 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5146 2.413) (end -2.5146 -2.413) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5146 2.286) (end 12.5984 2.286) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.5984 2.286) (end 12.5984 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start 12.5984 9.271) (end -2.5146 9.271) (layer F.SilkS) (width 0.15))
  (fp_line (start -2.5146 9.271) (end -2.5146 2.286) (layer F.SilkS) (width 0.15))
  (pad 1 thru_hole rect (at 0 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 2 thru_hole circle (at 2.5165 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 3 thru_hole circle (at 5.0165 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 4 thru_hole circle (at 7.5165 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (pad 5 thru_hole circle (at 10.0165 0) (size 2 2) (drill 1.2) (layers *.Cu *.Mask F.SilkS))
  (model Connect.3dshapes/Wafer_Horizontal15x5.8x7RM2.5-5.wrl
    (at (xyz 0 0 0))
    (scale (xyz 4 4 4))
    (rotate (xyz 0 0 0))
  )
)
