(export (version D)
  (design
    (source C:/Users/Esposch/Documents/GitHub/Labrador/PCB/Tinylab_proto1.sch)
    (date "9/05/2017 4:52:55 PM")
    (tool "Eeschema 4.0.4-stable")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source Tinylab_proto1.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref U2)
      (value LM324)
      (footprint Housings_SOIC:SOIC-14_3.9x8.7mm_Pitch1.27mm)
      (libsource (lib Tinylab_proto1-rescue) (part LM324-RESCUE-Tinylab_proto1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CA87E2))
    (comp (ref IC1)
      (value ATXMEGA32A4U-AU)
      (footprint Housings_QFP:LQFP-44_10x10mm_Pitch0.8mm)
      (libsource (lib atmel) (part ATXMEGA16A4U-A))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CA8F25))
    (comp (ref P2)
      (value USB_OTG)
      (footprint Connect:USB_Micro-B_WIDE)
      (libsource (lib conn) (part USB_OTG))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CA90D2))
    (comp (ref U1)
      (value 78L05)
      (footprint SMD:SOT-23-3)
      (libsource (lib Tinylab_proto1-rescue) (part 78L05-RESCUE-Tinylab_proto1))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CA99FA))
    (comp (ref R1)
      (value 1M)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAAB95))
    (comp (ref R3)
      (value 75K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAABF4))
    (comp (ref R5)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAAC5F))
    (comp (ref R6)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAACD2))
    (comp (ref R4)
      (value 75K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAAD11))
    (comp (ref R2)
      (value 1M)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAAD4C))
    (comp (ref C2)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAB4DE))
    (comp (ref C1)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CAB611))
    (comp (ref C3)
      (value C_Small)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CB13E1))
    (comp (ref C4)
      (value C_Small)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CB147C))
    (comp (ref R22)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CB4680))
    (comp (ref C13)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CB630B))
    (comp (ref R24)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CB9020))
    (comp (ref R11)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBCD2A))
    (comp (ref R7)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBCDA5))
    (comp (ref R13)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBE0F4))
    (comp (ref R9)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBE16B))
    (comp (ref R14)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBE21C))
    (comp (ref R10)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBE2C7))
    (comp (ref R12)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBE362))
    (comp (ref R8)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBE401))
    (comp (ref P3)
      (value DIG_OUT)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 55CBF4D5))
    (comp (ref C5)
      (value C_Small)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55D60181))
    (comp (ref U4)
      (value DMN63D8LDW)
      (footprint TO_SOT_Packages_SMD:SOT-363)
      (libsource (lib ESPO_PART) (part DMN63D8LDW))
      (sheetpath (names /) (tstamps /))
      (tstamp 55D6ACFD))
    (comp (ref P8)
      (value DIG_IN)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 55D6DB77))
    (comp (ref F1)
      (value F_Small)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part F_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 55D739F3))
    (comp (ref L1)
      (value INDUCTOR)
      (footprint Special_inductor:SMALL_INDUCTOR)
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 5606EE9E))
    (comp (ref D1)
      (value D_Schottky)
      (footprint Diodes_SMD:SMA_Standard)
      (libsource (lib device) (part D_Schottky))
      (sheetpath (names /) (tstamps /))
      (tstamp 5606FDB4))
    (comp (ref C9)
      (value CP1)
      (footprint Capacitors_SMD:c_elec_4x5.3)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 560719D9))
    (comp (ref C10)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 56071A50))
    (comp (ref C16)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5607355F))
    (comp (ref C15)
      (value CP1)
      (footprint Capacitors_SMD:c_elec_4x5.3)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 560735FE))
    (comp (ref P4)
      (value PDI/3V3)
      (footprint Pin_Headers:Pin_Header_Straight_2x02)
      (libsource (lib conn) (part CONN_02X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 56069A87))
    (comp (ref R23)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 566DE721))
    (comp (ref R25)
      (value 28R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 566DE7E8))
    (comp (ref C14)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 566DF655))
    (comp (ref P6)
      (value DAC_OUT)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 566DF832))
    (comp (ref R26)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 566E5C29))
    (comp (ref R27)
      (value 100R)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 566E5CBE))
    (comp (ref C6)
      (value CP1)
      (footprint Capacitors_SMD:c_elec_4x5.3)
      (libsource (lib device) (part CP1))
      (sheetpath (names /) (tstamps /))
      (tstamp 566F5A75))
    (comp (ref R19)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56AECD86))
    (comp (ref C11)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 5608B4BE))
    (comp (ref C8)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 56AF91A3))
    (comp (ref R17)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56AFE83E))
    (comp (ref R18)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56AFE8F3))
    (comp (ref U3)
      (value DMN63D8LDW)
      (footprint TO_SOT_Packages_SMD:SOT-363)
      (libsource (lib ESPO_PART) (part DMN63D8LDW))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B012DD))
    (comp (ref R20)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B0C682))
    (comp (ref R15)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B0C779))
    (comp (ref R16)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56B0C86E))
    (comp (ref L2)
      (value INDUCTOR)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E88440))
    (comp (ref L3)
      (value INDUCTOR)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E8DA35))
    (comp (ref C7)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E8E263))
    (comp (ref R21)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E9851A))
    (comp (ref R28)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E985EF))
    (comp (ref R29)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E9888A))
    (comp (ref R30)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 56E98921))
    (comp (ref P7)
      (value PSU)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 56F2A93D))
    (comp (ref L4)
      (value INDUCTOR)
      (footprint Resistors_SMD:R_1206)
      (libsource (lib device) (part INDUCTOR))
      (sheetpath (names /) (tstamps /))
      (tstamp 573254B0))
    (comp (ref C18)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57564580))
    (comp (ref C17)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 57564635))
    (comp (ref R31)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R))
      (sheetpath (names /) (tstamps /))
      (tstamp 5804605C))
    (comp (ref Q1)
      (value Q_NMOS_GSD)
      (footprint SMD:SOT-23-3)
      (libsource (lib device) (part Q_NMOS_GSD))
      (sheetpath (names /) (tstamps /))
      (tstamp 583120F2))
    (comp (ref D2)
      (value LED)
      (footprint LEDs:LED_0603)
      (libsource (lib device) (part LED))
      (sheetpath (names /) (tstamps /))
      (tstamp 5833E159))
    (comp (ref R32)
      (value 1K)
      (footprint Resistors_SMD:R_0603)
      (libsource (lib device) (part R_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 5833E34C))
    (comp (ref P10)
      (value EXPANSION)
      (footprint Pin_Headers:Pin_Header_Straight_1x03)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 5837847B))
    (comp (ref P11)
      (value SWITCH)
      (footprint Pin_Headers:Pin_Header_Straight_1x03)
      (libsource (lib conn) (part CONN_01X03))
      (sheetpath (names /) (tstamps /))
      (tstamp 58378536))
    (comp (ref P1)
      (value SCOPE_OUT)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 5832064B))
    (comp (ref P5)
      (value SCOPE_OUT)
      (footprint Pin_Headers:Pin_Header_Straight_1x04)
      (libsource (lib conn) (part CONN_01X04))
      (sheetpath (names /) (tstamps /))
      (tstamp 58320706))
    (comp (ref C12)
      (value C)
      (footprint Capacitors_SMD:C_0603)
      (libsource (lib device) (part C))
      (sheetpath (names /) (tstamps /))
      (tstamp 588029E7))
    (comp (ref F2)
      (value F_Small)
      (footprint Capacitors_SMD:C_1210)
      (libsource (lib device) (part F_Small))
      (sheetpath (names /) (tstamps /))
      (tstamp 58F5AF9C))
    (comp (ref P9)
      (value FUSE_BYPASS)
      (footprint Pin_Headers:Pin_Header_Straight_1x02)
      (libsource (lib conn) (part CONN_01X02))
      (sheetpath (names /) (tstamps /))
      (tstamp 58FEDB8C)))
  (libparts
    (libpart (lib Tinylab_proto1-rescue) (part 78L05-RESCUE-Tinylab_proto1)
      (fields
        (field (name Reference) U)
        (field (name Value) 78L05-RESCUE-Tinylab_proto1))
      (pins
        (pin (num 1) (name GND) (type input))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type input))))
    (libpart (lib atmel) (part ATXMEGA16A4U-A)
      (aliases
        (alias ATXMEGA32A4U-A)
        (alias ATXMEGA64A4U-A)
        (alias ATXMEGA128A4U-A))
      (description "TQFP44, 16k Flash, 4k Boot, 2k SRAM, 1k EEPROM, JTAG, USB")
      (docs http://www.atmel.com/Images/Atmel-8387-8-and16-bit-AVR-Microcontroller-XMEGA-A4U_Datasheet.pdf)
      (fields
        (field (name Reference) IC)
        (field (name Value) ATXMEGA16A4U-A)
        (field (name Footprint) TQFP44))
      (pins
        (pin (num 1) (name AC5/ADC5/PA5) (type BiDi))
        (pin (num 2) (name AC1OUT/AC6/ADC6/PA6) (type BiDi))
        (pin (num 3) (name AC0OUT/AC7/ADC7/PA7) (type BiDi))
        (pin (num 4) (name AREFB/ADC8/PB0) (type BiDi))
        (pin (num 5) (name ADC9/PB1) (type BiDi))
        (pin (num 6) (name DAC0/ADC10/PB2) (type BiDi))
        (pin (num 7) (name DAC1/ACD11/PB3) (type BiDi))
        (pin (num 8) (name GND) (type power_in))
        (pin (num 9) (name VCC) (type power_in))
        (pin (num 10) (name SDAIN/SDA/~OC0ALS~/OC0A/PC0) (type BiDi))
        (pin (num 11) (name SCLIN/SCL/XCK0/OC0AHS/OC0B/PC1) (type BiDi))
        (pin (num 12) (name SDAOUT/RXD0/~OC0BLS~/OC0C/PC2) (type BiDi))
        (pin (num 13) (name SCLOUT/TXD0/OC0BHS/OC0D/PC3) (type BiDi))
        (pin (num 14) (name ~SS~/~OC0CLS~/OC1A/PC4) (type BiDi))
        (pin (num 15) (name MOSI/XCK1/OC0CHS/OC1B/PC5) (type BiDi))
        (pin (num 16) (name CLKRTC/MISO/RXD1/~OC0DLS~/PC6) (type BiDi))
        (pin (num 17) (name EVOUT/CLKOUT/SCK/TXD1/OC0DHS/PC7) (type BiDi))
        (pin (num 18) (name GND) (type power_in))
        (pin (num 19) (name VCC) (type power_in))
        (pin (num 20) (name PD0/OC0A) (type BiDi))
        (pin (num 21) (name PD1/OC0B/XCK0) (type BiDi))
        (pin (num 22) (name PD2/OC0C/RXD0) (type BiDi))
        (pin (num 23) (name PD3/OC0D/TXD0) (type BiDi))
        (pin (num 24) (name PD4/OC1A/~SS~) (type BiDi))
        (pin (num 25) (name PD5/OC1B/XCK1/MOSI) (type BiDi))
        (pin (num 26) (name PD6/D-/RXD1/MISO) (type BiDi))
        (pin (num 27) (name PD7/D+/TXD1/SCK/CLKOUT/EVOUT) (type BiDi))
        (pin (num 28) (name PE0/OC0A/SDA) (type BiDi))
        (pin (num 29) (name PE1/OC0B/XCK0/SCL) (type BiDi))
        (pin (num 30) (name GND) (type power_in))
        (pin (num 31) (name VCC) (type power_in))
        (pin (num 32) (name PE2/OC0C/RXD0) (type BiDi))
        (pin (num 33) (name PE3/OC0D/TXD0) (type BiDi))
        (pin (num 34) (name PDI_DATA) (type input))
        (pin (num 35) (name ~RESET~/PDI_CLK) (type input))
        (pin (num 36) (name PR0/XTAL2/TOSC2) (type BiDi))
        (pin (num 37) (name PR1/XTAL1/TOSC1) (type BiDi))
        (pin (num 38) (name GND) (type power_in))
        (pin (num 39) (name AVCC) (type power_in))
        (pin (num 40) (name AREFA/AC0/ADC0/PA0) (type BiDi))
        (pin (num 41) (name AC1/ADC1/PA1) (type BiDi))
        (pin (num 42) (name AC2/ADC2/PA2) (type BiDi))
        (pin (num 43) (name AC3/ADC3/PA3) (type BiDi))
        (pin (num 44) (name AC4/ADC4/PA4) (type BiDi))))
    (libpart (lib device) (part C)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part CONN_01X02)
      (description "Connector, single row, 01x02")
      (footprints
        (fp Pin_Header_Straight_1X02)
        (fp Pin_Header_Angled_1X02)
        (fp Socket_Strip_Straight_1X02)
        (fp Socket_Strip_Angled_1X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))))
    (libpart (lib conn) (part CONN_01X03)
      (description "Connector, single row, 01x03")
      (footprints
        (fp Pin_Header_Straight_1X03)
        (fp Pin_Header_Angled_1X03)
        (fp Socket_Strip_Straight_1X03)
        (fp Socket_Strip_Angled_1X03))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X03))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))))
    (libpart (lib conn) (part CONN_01X04)
      (description "Connector, single row, 01x04")
      (footprints
        (fp Pin_Header_Straight_1X04)
        (fp Pin_Header_Angled_1X04)
        (fp Socket_Strip_Straight_1X04)
        (fp Socket_Strip_Angled_1X04))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_01X04))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib conn) (part CONN_02X02)
      (description "Connector, double row, 02x02")
      (footprints
        (fp Pin_Header_Straight_2X02)
        (fp Pin_Header_Angled_2X02)
        (fp Socket_Strip_Straight_2X02)
        (fp Socket_Strip_Angled_2X02))
      (fields
        (field (name Reference) P)
        (field (name Value) CONN_02X02))
      (pins
        (pin (num 1) (name P1) (type passive))
        (pin (num 2) (name P2) (type passive))
        (pin (num 3) (name P3) (type passive))
        (pin (num 4) (name P4) (type passive))))
    (libpart (lib device) (part CP1)
      (description "Polarised capacitor")
      (footprints
        (fp SMD*_Pol)
        (fp C_Axial*)
        (fp C_Radial*)
        (fp c_elec*)
        (fp C*elec)
        (fp TantalC*)
        (fp CP*))
      (fields
        (field (name Reference) C)
        (field (name Value) CP1))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part C_Small)
      (description "Unpolarized capacitor")
      (footprints
        (fp C?)
        (fp C_????_*)
        (fp C_????)
        (fp SMD*_c)
        (fp Capacitor*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib ESPO_PART) (part DMN63D8LDW)
      (fields
        (field (name Reference) U)
        (field (name Value) DMN63D8LDW))
      (pins
        (pin (num 1) (name S1) (type input))
        (pin (num 2) (name G1) (type input))
        (pin (num 3) (name D2) (type input))
        (pin (num 4) (name S2) (type input))
        (pin (num 5) (name G2) (type input))
        (pin (num 6) (name D1) (type input))))
    (libpart (lib device) (part D_Schottky)
      (description "Diode schottky")
      (footprints
        (fp D-Pak_TO252AA)
        (fp Diode_*)
        (fp *SingleDiode)
        (fp *SingleDiode*)
        (fp *_Diode_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib device) (part F_Small)
      (description Fuse)
      (footprints
        (fp CP*)
        (fp SM*))
      (fields
        (field (name Reference) F)
        (field (name Value) F_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part INDUCTOR)
      (footprints
        (fp Choke_*)
        (fp *Coil*))
      (fields
        (field (name Reference) L)
        (field (name Value) INDUCTOR))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib device) (part LED)
      (footprints
        (fp LED-*)
        (fp LED_*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Tinylab_proto1-rescue) (part LM324-RESCUE-Tinylab_proto1)
      (fields
        (field (name Reference) U)
        (field (name Value) LM324-RESCUE-Tinylab_proto1))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V+) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name ~) (type output))
        (pin (num 9) (name -) (type input))
        (pin (num 10) (name +) (type input))
        (pin (num 11) (name V-) (type power_in))
        (pin (num 12) (name +) (type input))
        (pin (num 13) (name -) (type input))
        (pin (num 14) (name ~) (type output))))
    (libpart (lib device) (part Q_NMOS_GSD)
      (description "Transistor N-MOSFET (general)")
      (fields
        (field (name Reference) Q)
        (field (name Value) Q_NMOS_GSD))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib device) (part R)
      (description Resistor)
      (footprints
        (fp R_*)
        (fp Resistor_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib device) (part R_Small)
      (description Resistor)
      (footprints
        (fp Resistor_*)
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib conn) (part USB_OTG)
      (description "USB micro/mini connector")
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) P)
        (field (name Value) USB_OTG))
      (pins
        (pin (num 1) (name VCC) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type power_in))
        (pin (num 5) (name GND) (type power_in))
        (pin (num 6) (name shield) (type passive)))))
  (libraries
    (library (logical conn)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\conn.lib"))
    (library (logical Tinylab_proto1-rescue)
      (uri C:\Users\Esposch\Documents\GitHub\Labrador\PCB\Tinylab_proto1-rescue.lib))
    (library (logical atmel)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\atmel.lib"))
    (library (logical device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library\\device.lib"))
    (library (logical ESPO_PART)
      (uri C:\Users\Esposch\Documents\KiCAD\ESPO_PART.lib)))
  (nets
    (net (code 1) (name /VCC_3V3)
      (node (ref U1) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C11) (pin 1))
      (node (ref F1) (pin 2))
      (node (ref IC1) (pin 19))
      (node (ref L2) (pin 1))
      (node (ref IC1) (pin 31))
      (node (ref C4) (pin 1)))
    (net (code 2) (name /TO_B1)
      (node (ref IC1) (pin 5))
      (node (ref U3) (pin 5)))
    (net (code 3) (name /V_minus_dac_out2)
      (node (ref R20) (pin 2))
      (node (ref R15) (pin 1))
      (node (ref R16) (pin 1))
      (node (ref U2) (pin 13)))
    (net (code 4) (name /S-Gen_Drain_Top_CH1)
      (node (ref U3) (pin 3))
      (node (ref R18) (pin 2))
      (node (ref R17) (pin 2)))
    (net (code 5) (name /Scope_Buffer_Input_CH1)
      (node (ref R3) (pin 1))
      (node (ref R1) (pin 1))
      (node (ref U2) (pin 3)))
    (net (code 6) (name /Scope_Buffer_Input_CH2)
      (node (ref U2) (pin 5))
      (node (ref R2) (pin 1))
      (node (ref R4) (pin 2)))
    (net (code 7) (name /D1_OUT)
      (node (ref R8) (pin 2))
      (node (ref P3) (pin 3)))
    (net (code 8) (name /PDI_CLK)
      (node (ref IC1) (pin 34))
      (node (ref P4) (pin 2)))
    (net (code 9) (name /PDI_DATA)
      (node (ref P4) (pin 4))
      (node (ref IC1) (pin 35)))
    (net (code 10) (name /3V3_OUT)
      (node (ref F1) (pin 1))
      (node (ref P4) (pin 1)))
    (net (code 11) (name /Switch_OC)
      (node (ref P11) (pin 1)))
    (net (code 12) (name /Scope_CH2_DC)
      (node (ref P5) (pin 3))
      (node (ref P5) (pin 1))
      (node (ref P5) (pin 4))
      (node (ref R2) (pin 2))
      (node (ref C2) (pin 1)))
    (net (code 13) (name /Scoe_CH1_AC)
      (node (ref C1) (pin 2))
      (node (ref P1) (pin 2)))
    (net (code 14) (name /Scope_CH2_AC)
      (node (ref P5) (pin 2))
      (node (ref C2) (pin 2)))
    (net (code 15) (name /S-Gen_CH1_DC)
      (node (ref C13) (pin 2))
      (node (ref R24) (pin 1))
      (node (ref P6) (pin 1)))
    (net (code 16) (name /S-Gen_CH1_AC)
      (node (ref C13) (pin 1))
      (node (ref P6) (pin 2)))
    (net (code 17) (name /S-Gen_CH2_DC)
      (node (ref R25) (pin 1))
      (node (ref C14) (pin 2))
      (node (ref P6) (pin 3)))
    (net (code 18) (name /S-Gen_CH2_AC)
      (node (ref C14) (pin 1))
      (node (ref P6) (pin 4)))
    (net (code 19) (name /PSU_FDBK)
      (node (ref IC1) (pin 1))
      (node (ref R27) (pin 1))
      (node (ref P10) (pin 2))
      (node (ref R26) (pin 2)))
    (net (code 20) (name /QTop)
      (node (ref D1) (pin 2))
      (node (ref L1) (pin 1))
      (node (ref Q1) (pin 3)))
    (net (code 21) (name /D0_MID)
      (node (ref R11) (pin 2))
      (node (ref R7) (pin 1)))
    (net (code 22) (name /D1_MID)
      (node (ref R8) (pin 1))
      (node (ref R12) (pin 2)))
    (net (code 23) (name /D2_MID)
      (node (ref R13) (pin 2))
      (node (ref R9) (pin 1)))
    (net (code 24) (name /D3_MID)
      (node (ref R14) (pin 2))
      (node (ref R10) (pin 1)))
    (net (code 25) (name /L-Ana_IN_CH1)
      (node (ref P8) (pin 1))
      (node (ref U4) (pin 5)))
    (net (code 26) (name /R22-R24)
      (node (ref R22) (pin 1))
      (node (ref R24) (pin 2)))
    (net (code 27) (name /PSU_OUT)
      (node (ref P11) (pin 3))
      (node (ref P7) (pin 1))
      (node (ref R32) (pin 1)))
    (net (code 28) (name "Net-(L3-Pad1)")
      (node (ref L4) (pin 2))
      (node (ref L3) (pin 1)))
    (net (code 29) (name /CH1)
      (node (ref R21) (pin 1))
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 1))
      (node (ref IC1) (pin 42)))
    (net (code 30) (name /CH2)
      (node (ref R28) (pin 2))
      (node (ref IC1) (pin 2))
      (node (ref IC1) (pin 40))
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 6)))
    (net (code 31) (name /DAC_OUT)
      (node (ref U2) (pin 10))
      (node (ref IC1) (pin 6)))
    (net (code 32) (name "Net-(F2-Pad2)")
      (node (ref L1) (pin 2))
      (node (ref F2) (pin 2))
      (node (ref P9) (pin 2)))
    (net (code 33) (name /L-Ana_IN_CH2)
      (node (ref P8) (pin 2))
      (node (ref U4) (pin 2)))
    (net (code 34) (name /DIG_CH1)
      (node (ref U4) (pin 6))
      (node (ref IC1) (pin 15)))
    (net (code 35) (name /AVCC)
      (node (ref C5) (pin 1))
      (node (ref R5) (pin 1))
      (node (ref C17) (pin 1))
      (node (ref C8) (pin 1))
      (node (ref L2) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref IC1) (pin 39)))
    (net (code 36) (name /D2-prefuse)
      (node (ref R13) (pin 1))
      (node (ref IC1) (pin 32)))
    (net (code 37) (name /D1-prefuse)
      (node (ref IC1) (pin 29))
      (node (ref R12) (pin 1)))
    (net (code 38) (name /D0-prefuse)
      (node (ref R11) (pin 1))
      (node (ref IC1) (pin 28)))
    (net (code 39) (name +5V)
      (node (ref C3) (pin 1))
      (node (ref P9) (pin 1))
      (node (ref P2) (pin 1))
      (node (ref F2) (pin 1))
      (node (ref U1) (pin 3))
      (node (ref C10) (pin 1))
      (node (ref C9) (pin 1)))
    (net (code 40) (name /D-)
      (node (ref IC1) (pin 26))
      (node (ref P2) (pin 2)))
    (net (code 41) (name /D+)
      (node (ref P2) (pin 3))
      (node (ref IC1) (pin 27)))
    (net (code 42) (name /D3-OUT)
      (node (ref R10) (pin 2))
      (node (ref P3) (pin 1)))
    (net (code 43) (name /D2-OUT)
      (node (ref R9) (pin 2))
      (node (ref P3) (pin 2)))
    (net (code 44) (name /D0_OUT)
      (node (ref R7) (pin 2))
      (node (ref P3) (pin 4)))
    (net (code 45) (name /D3-prefuse)
      (node (ref IC1) (pin 33))
      (node (ref R14) (pin 1)))
    (net (code 46) (name /VGND)
      (node (ref R29) (pin 2))
      (node (ref R30) (pin 1))
      (node (ref P7) (pin 2))
      (node (ref D2) (pin 1))
      (node (ref C17) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref Q1) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref P10) (pin 3))
      (node (ref U1) (pin 1))
      (node (ref IC1) (pin 18))
      (node (ref IC1) (pin 38))
      (node (ref C12) (pin 2))
      (node (ref P2) (pin 5))
      (node (ref P2) (pin 6))
      (node (ref R21) (pin 2))
      (node (ref IC1) (pin 14))
      (node (ref R28) (pin 1))
      (node (ref U3) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref R27) (pin 2))
      (node (ref C9) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref U3) (pin 4))
      (node (ref C10) (pin 2))
      (node (ref C16) (pin 2))
      (node (ref C15) (pin 2))
      (node (ref P4) (pin 3))
      (node (ref R6) (pin 1))
      (node (ref C5) (pin 2))
      (node (ref IC1) (pin 30))
      (node (ref IC1) (pin 8))
      (node (ref U4) (pin 4))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 2))
      (node (ref U2) (pin 11))
      (node (ref U4) (pin 1)))
    (net (code 47) (name /Disconnected_USB)
      (node (ref P2) (pin 4)))
    (net (code 48) (name /DIG_CH2)
      (node (ref U4) (pin 3))
      (node (ref IC1) (pin 12)))
    (net (code 49) (name "Net-(IC1-Pad10)")
      (node (ref IC1) (pin 10)))
    (net (code 50) (name "Net-(IC1-Pad3)")
      (node (ref IC1) (pin 3)))
    (net (code 51) (name /DAC_OUT2)
      (node (ref U2) (pin 12))
      (node (ref IC1) (pin 7)))
    (net (code 52) (name "Net-(IC1-Pad9)")
      (node (ref IC1) (pin 9)))
    (net (code 53) (name "Net-(IC1-Pad20)")
      (node (ref IC1) (pin 20)))
    (net (code 54) (name /XCK)
      (node (ref IC1) (pin 17))
      (node (ref IC1) (pin 11)))
    (net (code 55) (name "Net-(IC1-Pad21)")
      (node (ref IC1) (pin 21)))
    (net (code 56) (name "Net-(IC1-Pad41)")
      (node (ref IC1) (pin 41)))
    (net (code 57) (name /OPAMP_VCC)
      (node (ref U2) (pin 4))
      (node (ref L4) (pin 1))
      (node (ref C16) (pin 1)))
    (net (code 58) (name "Net-(IC1-Pad22)")
      (node (ref IC1) (pin 22)))
    (net (code 59) (name "Net-(IC1-Pad37)")
      (node (ref IC1) (pin 37)))
    (net (code 60) (name /Scope_CH1_DC)
      (node (ref P1) (pin 3))
      (node (ref P1) (pin 1))
      (node (ref R1) (pin 2))
      (node (ref P1) (pin 4))
      (node (ref C1) (pin 1)))
    (net (code 61) (name "Net-(IC1-Pad13)")
      (node (ref IC1) (pin 13)))
    (net (code 62) (name "Net-(IC1-Pad23)")
      (node (ref IC1) (pin 23)))
    (net (code 63) (name "Net-(IC1-Pad43)")
      (node (ref IC1) (pin 43)))
    (net (code 64) (name /AVCC_ON_2)
      (node (ref R6) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref IC1) (pin 44))
      (node (ref R5) (pin 2))
      (node (ref R3) (pin 2)))
    (net (code 65) (name "Net-(IC1-Pad25)")
      (node (ref IC1) (pin 25)))
    (net (code 66) (name "Net-(IC1-Pad16)")
      (node (ref IC1) (pin 16)))
    (net (code 67) (name "Net-(IC1-Pad36)")
      (node (ref IC1) (pin 36)))
    (net (code 68) (name /PSU_Unfiltered_Raw)
      (node (ref R26) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref P10) (pin 1))
      (node (ref D1) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref L3) (pin 2))
      (node (ref P11) (pin 2)))
    (net (code 69) (name /Buffered_DAC_CH1)
      (node (ref R22) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref R19) (pin 1))
      (node (ref U2) (pin 8)))
    (net (code 70) (name /Buffered_DAC_CH2)
      (node (ref R20) (pin 1))
      (node (ref U2) (pin 14))
      (node (ref R23) (pin 2))
      (node (ref R30) (pin 2)))
    (net (code 71) (name /TO_B0)
      (node (ref U3) (pin 2))
      (node (ref IC1) (pin 4)))
    (net (code 72) (name /S-Gen_Drain_Top_CH2)
      (node (ref U3) (pin 6))
      (node (ref R16) (pin 2))
      (node (ref R15) (pin 2)))
    (net (code 73) (name /PSU_PWM)
      (node (ref Q1) (pin 1))
      (node (ref R31) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref IC1) (pin 24)))
    (net (code 74) (name "Net-(D2-Pad2)")
      (node (ref D2) (pin 2))
      (node (ref R32) (pin 2)))
    (net (code 75) (name /V_minus_dac_out)
      (node (ref R18) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref U2) (pin 9))
      (node (ref R19) (pin 2)))
    (net (code 76) (name /R23-R25)
      (node (ref R23) (pin 1))
      (node (ref R25) (pin 2)))))